{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Overview","CV9400","S 886 Series","8500 Series","840-846 Series","CG Series","NG304 Series"],"not_rendered":{"charts":0,"images":28,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Overview","index":0,"n_rows":124,"n_cols":9,"rows_kept":124,"cut":false,"hidden":false,"merged":[[61,0,61,8],[62,1,66,1],[62,4,66,4],[62,5,66,5],[62,7,66,7],[62,8,66,8],[68,1,72,1],[68,4,72,4],[68,5,72,5],[68,7,72,7],[68,8,72,8],[50,0,50,8],[51,1,53,1],[51,4,53,4],[51,5,53,5],[51,7,53,7],[51,8,53,8],[55,0,55,8],[56,1,59,1],[56,3,59,3],[56,4,59,4],[56,5,59,5],[56,7,59,7],[56,8,59,8],[46,7,48,7],[46,8,48,8],[40,0,40,8],[41,1,43,1],[41,4,43,4],[41,5,43,5],[41,7,43,7],[41,8,43,8],[45,0,45,8],[46,1,48,1],[46,4,48,4],[46,5,48,5],[20,7,27,7],[20,8,27,8],[20,1,27,1],[36,0,36,8],[37,1,38,1],[37,4,38,4],[37,5,38,5],[37,7,38,7],[37,8,38,8],[0,0,0,8],[7,0,7,8],[3,1,3,4],[74,0,74,8],[75,1,78,1],[75,4,78,4],[75,5,78,5],[75,7,78,7],[75,8,78,8],[8,1,17,1],[8,4,17,4],[8,5,17,5],[8,7,17,7],[8,8,17,8],[8,3,17,3],[19,0,19,8],[29,0,29,8],[30,1,34,1],[30,4,34,4],[30,5,34,5],[30,7,34,7],[30,8,34,8],[20,4,27,4],[20,5,27,5],[87,0,87,8],[88,1,91,1],[88,4,91,4],[88,5,91,5],[88,7,91,7],[88,8,91,8],[80,1,84,1],[80,4,84,4],[80,5,84,5],[80,7,84,7],[80,8,84,8],[105,0,105,8],[106,1,109,1],[106,4,109,4],[106,5,109,5],[106,7,109,7],[106,8,109,8],[93,0,93,8],[94,1,97,1],[94,4,97,4],[94,5,97,5],[94,7,97,7],[94,8,97,8],[99,0,99,8],[100,1,103,1],[100,4,103,4],[100,5,103,5],[100,7,103,7],[100,8,103,8],[117,0,117,8],[118,8,123,8],[118,7,123,7],[118,6,123,6],[118,5,123,5],[118,4,123,4],[118,1,123,1],[118,3,123,3],[111,0,111,8],[112,1,115,1],[112,4,115,4],[112,5,115,5],[112,7,115,7],[112,8,115,8],[112,6,115,6],[112,3,115,3],[112,2,115,2],[112,0,115,0]]}
["Overview RegO Check Valves"]
["Version","15-10-2020"]
[{"$nulls":7},"PSI","Bar"]
["Portfolio"," Piston Check Valves  -  Swing Check Valves  -  Inline Check Valves  -  Bronze  -  Stainless Steel",{"$nulls":4},"Calculator from PSI to Bar",1,{"$f":"H4/14.5038","v":6.8947448254940091E-2}]
[]
["Style","Product Picture","Inlet\nOutlet","Pressure Range","Gas","Liquid","Cv value","Certification","Remarks"]
[]
["Piston Check Valve 9400 Series  -  316 Stainless Steel Valve Body-Stem-Spring"]
["CV9404BW","\nClick picture for detailed info","1/2\"  Butt Weld","50 Bar\n\n720 PSIG\n\nClass 300 - PN50","   Oxygen\n   Nitrogen\n   Argon\nKrypton\n   CO2\n   Natural Gas\nEthane\nEthylene\n   Air\n   N2O","   Oxygen\n   Nitrogen\n   Argon\nKrypton\n   CO2\n   Natural Gas\nEthane\nEthylene\n   Air\n   N2O",5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nOpening Pressure - 0,1 Barg\n\n100% Factory Tested\n\nHigh CV - Conical Seat Design\n\nOne piece Seat Assembly - Zero small pieces\n\nEasy to construct to SK Globe Valve\n\nConnection - Butt Weld / Socket Weld / SCH.10"]
["CV9406BW",null,"3/4\"  Butt Weld",null,null,null,9.4]
["CV9408BW",null,"1\"  Butt Weld",null,null,null,14]
["CV9412BW",null,"1 1/2\"   Butt Weld",null,null,null,28.3]
["CV9416BW",null,"2\"  Butt Weld",null,null,null,53]
["CV9404SW",null,"1/2\"  Socket Weld",null,null,null,5]
["CV9406SW",null,"3/4\"  Socket Weld",null,null,null,9.4]
["CV9408SW",null,"1\"  Socket Weld",null,null,null,14]
["CV9412SW",null,"1 1/2\"   Socket Weld",null,null,null,28.3]
["CV9416SW",null,"2\"  Socket Weld",null,null,null,53]
[]
["Swing Check Valve 886 Series  -  PTFE Gasket Soft Seat  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886-4WA","\nClick picture for detailed info","1/2\"  Butt Weld","27.5 Bar\n400 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity\n\n\n\n"]
["S-886-8WA",null,"1\"  Butt Weld","27.5 Bar\n400 PSIG",null,null,18]
["S-886-12WA",null,"1 1/2\"   Butt Weld","27.5 Bar\n400 PSIG",null,null,61]
["S-886-16W3A",null,"2\"  Butt Weld","50 Bar\n720 PSIG",null,null,99]
["S-886-24WA",null,"3\"  Butt Weld","19 Bar\n275 PSIG",null,null,225]
["S-886-24WJ",null,"3\"  Butt Weld SCH.40","19 Bar\n275 PSIG",null,null,225]
["S-886-32WA",null,"4\"  Butt Weld","19 Bar\n275 PSIG",null,null,475]
["S-886-32W3J",null,"4\"  Butt Weld SCH.40","50 Bar\n720 PSIG",null,null,475]
[]
["Swing Check Valve 886 Series  -  PTFE Gasket - Metal Seat  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886M-16W3A","\nClick picture for detailed info","2\"  Butt Weld SCH.10","50 Bar\n720 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",99,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["S-886M-24W3A",null,"3\"  Butt Weld SCH.10","50 Bar\n720 PSIG",null,null,225]
["S-886M-24W3J",null,"3\"  Butt Weld SCH.40","50 Bar\n720 PSIG",null,null,225]
["S-886-32WA",null,"4\"  Butt Weld SCH.10","19 Bar\n275 PSIG",null,null,475]
["S-886-32W3J",null,"4\"  Butt Weld SCH.40","50 Bar\n720 PSIG",null,null,475]
[]
["Swing Check Valve 886 Series  -  Grafoil Gasket - Metal Seat - for Hydrogen Service  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886MGF-16W3A","\nClick picture for detailed info","2\"  Butt Weld","50 Bar\n720 PSIG","   Hydrogen             Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas","   Hydrogen             Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas",99,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["S-886MGF-24W3A",null,"3\"  Butt Weld","50 Bar\n720 PSIG",null,null,225]
[]
["Swing Check Valve 886 Series  -  PTFE Gasket Soft Seat  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886-4S","\nClick picture for detailed info","1/2\"  Socket Weld","27.5 Bar\n400 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["S-886-8S",null,"1\"  Socket Weld","27.5 Bar\n400 PSIG",null,null,18]
["S-886-12S",null,"1 1/2\"   Socket Weld","27.5 Bar\n400 PSIG",null,null,61]
[]
["Swing Check Valve 886 Series  -  PTFE Gasket Metal Seat  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886M-4S3","\nClick picture for detailed info","1/2\"  Socket Weld","50 Bar\n720 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["S-886M-8S3",null,"1\"  Socket Weld","50 Bar\n720 PSIG",null,null,18]
["S-886M-12S3",null,"1 1/2\"   Socket Weld","50 Bar\n720 PSIG",null,null,61]
[]
["Swing Check Valve 886 Series  -   Grafoil Gasket - SOFT Seat - for Hydrogen Service  -  316 Stainless Steel Valve Body-Cap-Arm"]
["S-886GF-4S","\nClick picture for detailed info","1/2\"  Socket Weld","27.5 Bar\n400 PSIG","   Hydrogen     Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas","   Hydrogen     Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity\n\nSeal Material Neoflon"]
["S-886GF-8S",null,"1\"  Socket Weld","27.5 Bar\n400 PSIG",null,null,18]
["S-886GF-12S",null,"1 1/2\"   Socket Weld","27.5 Bar\n400 PSIG",null,null,61]
[]
["Piston Check Valve 8500 Series  -  Bronze Valve Body - Brass Cap-Plunger"]
["BK8508S","\nClick picture for detailed info","1.128\" - 1.13\" Sil Braze","41.3 Barg\n\n600 PSIG\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\nEthane\nEthylene\n   Air\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\nEthane\nEthylene\n   Air\n",10,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,14 Barg\n\n100% Factory Tested\n\nHigh CV - Conical Seat Design\n\nOne piece Seat Assembly - Zero small pieces"]
["BK8508T",null,"1\"  Female NPT",null,null,null,10]
["BK85012S",null,"1.629\" - 1.631\" Sil Braze",null,null,null,27]
["BK85012T",null,"1 1/2\"   Female NPT",null,null,null,27]
[]
["Swing Check Valve 840 Series  -  Soft Seated  -  Bronze Valve Body"]
["B-840-4T","\nClick picture for detailed info","1/2\"  F. NPT","27.6 Bar\n400 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity                                                                                   PCTFE Seal"]
["B-840-6T",null,"3/4\"  F. NPT","27.6 Bar\n400 PSIG",null,null,7]
["B-840-8T",null,"1\"  F. NPT","27.6 Bar\n400 PSIG",null,null,10]
["B-840-12T",null,"1 1/2\"  F. NPT","27.6 Bar\n400 PSIG",null,null,40]
["B-840-16T",null,"2\"  F. NPT","27.6 Bar\n400 PSIG",null,null,100]
[]
["B-840-4S","\nClick picture for detailed info","1/2\" Sil Braze End","27.6 Bar\n400 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity                                                                                   PCTFE Seal"]
["B-840-6S",null,"3/4\" Sil Braze End","27.6 Bar\n400 PSIG",null,null,7]
["B-840-8S",null,"1\" Sil Braze End","27.6 Bar\n400 PSIG",null,null,10]
["B-840-12S",null,"1 1/2\" Sil Braze End","27.6 Bar\n400 PSIG",null,null,40]
["B-840-16S",null,"2\" Sil Braze End","27.6 Bar\n400 PSIG",null,null,100]
[]
["Swing Check Valve 846 Series  -  Metal Seated  -  Bronze Valve Body"]
["B-846M-4T6","\nClick picture for detailed info","1/2\"  F. NPT","42 Bar\n600 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity                                                                                                                                    "]
["B-846M-8T6",null,"1\"  F. NPT","42 Bar\n600 PSIG",null,null,10]
["B-846M-12T6",null,"1 1/2\"  F. NPT","42 Bar\n600 PSIG",null,null,40]
["B-846M-16T6",null,"2\"  F. NPT","42 Bar\n600 PSIG",null,null,100]
[]
["B-846M-4S6","\nClick picture for detailed info","1/2\" Sil Braze End","42 Bar\n600 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",4.5,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,03 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["B-846M-6S6",null,"3/4\" Sil Braze End","42 Bar\n600 PSIG",null,null,7]
["B-846M-8S6",null,"1\" Sil Braze End","42 Bar\n600 PSIG",null,null,10]
["B-846M-12S6",null,"1 1/2\" Sil Braze End","42 Bar\n600 PSIG",null,null,40]
["B-846M-16S6",null,"2\" Sil Braze End","42 Bar\n600 PSIG",null,null,100]
[]
[]
["Inline Check Valve CG Series  -  Metal Seated  -  Stainless Steel Valve "]
["CG-250SS","\nClick picture for detailed info","1/4\"  F. NPT","345 Bar\n5000 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",0.87,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,07 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["CG-375SS",null,"3-8\"  F. NPT","345 Bar\n5000 PSIG",null,null,2.2999999999999998]
["CG-500SS",null,"1/2\"  F. NPT","345 Bar\n5000 PSIG",null,null,3.5]
["CG-750SS",null,"3/4\"  F. NPT","345 Bar\n5000 PSIG",null,null,5.2]
[]
["Inline Check Valve CG Series  -  Soft Seated  -  Stainless Steel Valve "]
["CG-250SSL","\nClick picture for detailed info","1/4\"  F. NPT","17.2 Bar\n250 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",null,0.87,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,07 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity                                                                                      Viton Seal"]
["CG-375SSL",null,"3-8\"  F. NPT","17.2 Bar\n250 PSIG",null,null,2.2999999999999998]
["CG-500SSL",null,"1/2\"  F. NPT","138 Bar\n2000 PSIG",null,null,3.5]
["CG-750SSL",null,"3/4\"  F. NPT","138 Bar\n2000 PSIG",null,null,5.2]
[]
["Inline Check Valve CG Series  -  Metal Seated  -  Brass Valve "]
["CG-250B","\nClick picture for detailed info","1/4\"  F. NPT","207 Bar\n3000 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",0.87,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,07 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity"]
["CG-375B",null,"3-8\"  F. NPT","207 Bar\n3000 PSIG",null,null,2.2999999999999998]
["CG-500B",null,"1/2\"  F. NPT","207 Bar\n3000 PSIG",null,null,3.5]
["CG-750B",null,"3/4\"  F. NPT","207 Bar\n3000 PSIG",null,null,5.2]
[]
["Inline Check Valve CG Series  -  Soft Seated  -  Brass Valve "]
["CG-250SBL","\nClick picture for detailed info","1/4\"  F. NPT","17.2 Bar\n250 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",null,0.87,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\nLow Opening Pressure - 0,07 Barg\n\n100% Factory Tested\n\nHigh Flow Capacity                                                                                      Viton Seal"]
["CG-375BL",null,"3-8\"  F. NPT","17.2 Bar\n250 PSIG",null,null,2.2999999999999998]
["CG-500BL",null,"1/2\"  F. NPT","138 Bar\n2000 PSIG",null,null,3.5]
["CG-750BL",null,"3/4\"  F. NPT","138 Bar\n2000 PSIG",null,null,5.2]
[]
["Inline Check Valve NG304 Series  -  Brass Valve "]
["NG304","\nClick picture for detailed info","1/2\"-14  F. NPT","69 Bar\n1000 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",null,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\n100% Factory Tested\n"]
[]
[]
[]
[]
["Inline Check Valve NG304 Series  -  Stainless Steel Valve "]
["NG304SSA","\nClick picture for detailed info","M36x2  Male","69 Bar\n1000 PSIG","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n","   Oxygen\n   Nitrogen\n   Argon\n   CO2\n   Natural Gas\n",null,"PED\n\nCE Marking\n","Cleaned and packaged for Oxygen Service per CGA G-4.1\n\n100% Factory Tested\n"]
["NG304SSB",null,"M30x1.5  Male"]
["NG304SSC",null,"1/2\"-14  F. NPT"]
["NG304SSAP",null,"M36x2  Male"]
["NG304SSBP",null,"M30x1.5  Male"]
["NG304SSCP",null,"1/2\"-14  F. NPT"]

{"sheet":"CV9400","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"S 886 Series","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"8500 Series","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"840-846 Series","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"CG Series","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"NG304 Series","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}