{"text_format":"2","workbook":"xlsx","n_sheets":7,"sheets":["Overview","110 Series","110WHZ Series","110 LOX Series","302-306 Series","310-310X Series","322 & 326 Series"],"not_rendered":{"charts":0,"images":32,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Overview","index":0,"n_rows":95,"n_cols":12,"rows_kept":95,"cut":false,"hidden":false,"merged":[[76,1,78,1],[80,0,80,11],[81,0,89,0],[81,1,87,1],[81,3,87,3],[81,5,89,5],[81,6,89,6],[81,7,89,7],[81,8,89,8],[81,9,89,9],[81,10,89,10],[81,11,89,11],[88,1,89,1],[88,3,89,3],[76,0,78,0],[76,5,79,5],[76,6,79,6],[76,7,79,7],[76,8,79,8],[76,9,79,9],[76,10,79,10],[76,11,79,11],[90,0,94,0],[90,1,94,1],[29,5,38,5],[29,6,38,6],[29,7,38,7],[29,8,38,8],[29,9,38,9],[29,10,38,10],[29,11,38,11],[62,0,62,11],[51,0,51,11],[52,6,61,6],[52,1,58,1],[59,1,61,1],[52,3,58,3],[59,3,61,3],[63,0,66,0],[63,1,66,1],[63,3,66,3],[63,5,66,5],[63,6,66,6],[63,7,66,7],[63,8,66,8],[63,9,66,9],[63,10,66,10],[63,11,66,11],[72,10,74,10],[72,11,74,11],[72,6,74,6],[72,7,74,7],[72,8,74,8],[72,9,74,9],[75,0,75,11],[68,0,70,0],[68,5,70,5],[68,6,70,6],[68,7,70,7],[68,8,70,8],[68,9,70,9],[68,10,70,10],[68,11,70,11],[69,1,70,1],[69,3,70,3],[67,0,67,11],[72,5,74,5],[72,0,74,0],[90,6,94,6],[90,3,94,3],[90,5,94,5],[90,7,94,7],[90,8,94,8],[90,9,94,9],[90,10,94,10],[90,11,94,11],[26,8,27,8],[26,9,27,9],[26,10,27,10],[26,11,27,11],[71,0,71,11],[72,1,74,1],[72,3,73,3],[40,6,50,6],[52,0,61,0],[52,5,61,5],[52,7,61,7],[52,8,61,8],[52,9,61,9],[52,10,61,10],[52,11,61,11],[39,0,39,11],[0,0,0,11],[7,3,12,3],[7,5,12,5],[7,7,12,7],[7,8,12,8],[7,9,12,9],[7,10,12,10],[7,11,12,11],[7,0,12,0],[6,0,6,11],[3,1,3,4],[13,3,20,3],[13,5,20,5],[13,7,20,7],[13,8,20,8],[13,9,20,9],[13,10,20,10],[13,11,20,11],[21,8,25,8],[21,9,25,9],[21,10,25,10],[21,11,25,11],[29,0,34,0],[29,1,34,1],[35,0,38,0],[35,1,38,1],[35,3,38,3],[7,1,12,1],[13,1,20,1],[21,1,25,1],[26,1,27,1],[28,0,28,11],[8,6,12,6],[17,6,20,6],[13,6,16,6],[26,0,27,0],[26,3,27,3],[26,5,27,5],[26,6,27,6],[26,7,27,7],[21,0,25,0],[21,3,25,3],[21,5,25,5],[21,6,25,6],[21,7,25,7],[13,0,20,0],[40,0,50,0],[40,5,50,5],[40,7,50,7],[40,8,50,8],[40,9,50,9],[40,10,50,10],[40,11,50,11],[44,1,50,1],[40,1,43,1]]}
["Overview RegO Gate Valve"]
["Version","16-9-2020"]
[{"$nulls":10},"PSI","Bar"]
["Portfolio","           Stainless Steel and Bronz Gate Valves - Special LOX Gate Valves",{"$nulls":7},"Calculator from PSI to Bar",720,{"$f":"K4/14.5038","v":49.64216274355686}]
[]
[null,"Product Pictures","Size","Connection","Stem Lenght","Temperature \nRating","Pressure \nRating","Gas","Liquid","Certificate","Applications","Remarks"]
["    110 Series Gate Valve with End Connections:  Flange  -  Butt Weld  -  Socket Weld  -  Threaded end.          Flange on stem for Foam Insulation available on request. "]
["\n\n110 Series\nStainless Steel ","\nClick picture for detailed info","1\"","RF Flange","451 mm","-196°C \n\nto \n\n+65°C","19 Bar\nClass 150","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n   Material: \n   Body and Bonnet \n   Stainless Steel\n   ASTM A351-CF8 J92600\n\n   PCTFE seat provides a \n   bubble tight seal and is    \n   replaceable.\n\n "]
[null,null,"\n1 1/2\"\n",null,"556 mm",null,"19 Bar\nClass 150\n\nand\n\n50 Bar\nClass 300"]
[null,null,"\n2\"\n",null,"556 mm"]
[null,null,"3\"",null,"800 mm"]
[null,null,"4\"",null,"857 mm"]
[null,null,"6\"",null,"1054 mm"]
["\n\n110 Series\nStainless Steel ","\nClick picture for detailed info","1/2\"","Butt Weld\nSCH.10\nSCH.40","451 mm","-196°C \n\nto \n\n+65°C","19 Bar\nClass 150","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   \n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n   Material: \n   Body and Bonnet \n   Stainless Steel\n   ASTM A351-CF8 J92600\n\n   PCTFE seat provides a \n   bubble tight seal and is    \n   replaceable.\n\n "]
[null,null,"3/4\"",null,"451 mm"]
[null,null,"1\"",null,"451 mm"]
[null,null,"\n1 1/2\"\n",null,"556 mm"]
[null,null,"\n2\"\n",null,"556 mm",null,"19 Bar\nClass 150\n\nand\n\n50 Bar\nClass 300"]
[null,null,"3\"",null,"800 mm"]
[null,null,"4\"",null,"857 mm"]
[null,null,"6\"",null,"1054 mm"]
["\n\n110 Series\nStainless Steel ","\nClick picture for detailed info","1/2\"","Socket Weld","451 mm","-196°C \n\nto \n\n+65°C","19 Bar\nClass 150\n\nand\n\n50 Bar\nClass 300","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   Cleaned for use in \n   Oxygen per CGA G-4.1\n   100% Factory Tested\n   \n   Material: Body and Bonnet \n   Stainless Steel\n   ASTM A351-CF8 J92600\n   \n   PCTFE seat provides a \n   bubble tight seal and is    \n   replaceable."]
[null,null,"3/4\"",null,"451 mm"]
[null,null,"1\"",null,"451 mm"]
[null,null,"\n1 1/2\"\n",null,"556 mm"]
[null,null,"\n2\"\n",null,"556 mm"]
["110 Series\nStainless Steel ","\nClick picture for detailed info","1/2\"","Threaded","451 mm","-196°C \n\nto \n\n+65°C","19 Bar\nClass 150","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   Cleaned for use in \n   Oxygen per CGA G-4.1\n   100% Factory Tested\n   \n   Material: Body and Bonnet \n   Stainless Steel\n   ASTM A351-CF8 J92600\n   PCTFE seat provides a \n   bubble tight seal and is    \n   replaceable.\n\n "]
[null,null,"1\"",null,"451 mm"]
["   110 WHZ Series Gate Valve with End Connections:  Butt Weld  -  Socket Weld.          Special Grafoil stem packing.          Flange on stem for Foam Insulation available on request. "]
["\n110 WHZ Series\nStainless Steel","\nClick picture for detailed info","\n2\"\n","Butt Weld\nSCH.10","556 mm","-196°C \n\nto \n\n+65°C","19 Bar\nClass 150\n\nand\n\n50 Bar\nClass 300","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   \n\n   Special Grafoil \n   Stem packing\n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n   100% Factory Tested\n   \n   Material and Seat,\n   same as all above\n\n "]
[null,null,"\n2\"\n","Butt Weld\nSCH.40","556 mm"]
[null,null,"3\"","Butt Weld\nSCH.10","800 mm"]
[null,null,"4\"","Butt Weld\nSCH.10","857 mm"]
[null,null,"6\"","Butt Weld\nSCH.10","1054 mm"]
[null,null,"6\"","Butt Weld\nSCH.40","1054 mm"]
["\n110 WHZ Series\nStainless Steel","\nClick picture for detailed info","1/2\"","Socket Weld","451 mm"]
[null,null,"3/4\"",null,"451 mm"]
[null,null,"1\"",null,"451 mm"]
[null,null,"\n1 1/2\"\n",null,"556 mm"]
["   110 LOX Series Gate Valve - Specifically designed for use with Liquide Oxygen.          Flange on stem for Foam Insulation available on request.          Flange and Threaded end connections available on request. "]
["\n\n110 LOX \nSeries\n\nStainless Steel ","\nClick picture for detailed info","1/2\"","Socket Weld","451 mm","-196°C \n\nto \n\n+65°C","50 Bar\n\nClass 300","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","ASU Plants Piping Systems\nSkids","   \n\n   Specifically designed for \n   use with Liquid Oxygen.\n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n   Material: \n   Body and Bonnet \n   Stainless Steel\n   ASTM A351-CF8 J92600\n\n   PCTFE seat provides a \n   bubble tight seal and is    \n   replaceable.\n\n   Grafoil Stem Packing \n   available as option\n\n "]
[null,null,"3/4\"","Socket Weld","451 mm"]
[null,null,"1\"","Socket Weld","451 mm"]
[null,null,"\n1 1/2\"\n","Socket Weld","556 mm"]
[null,"Click picture for detailed info","\n2\"\n","Butt Weld\nSCH.10","556 mm"]
[null,null,"3\"","Butt Weld\nSCH.10","800 mm"]
[null,null,"3\"","Butt Weld\nSCH.10","800 mm"]
[null,null,"4\"","Butt Weld\nSCH.10","857 mm"]
[null,null,"4\"","Butt Weld\nSCH.40","857 mm"]
[null,null,"6\"","Butt Weld\nSCH.10","1054 mm"]
[null,null,"6\"","Butt Weld\nSCH.40","1054 mm"]
["    302 Series Bronze Gate Valve - Non Extended Stem, Metal Seated, with End Connections:  Silver Braze Ends  -  Threaded Ends  -  Stainless Steel Pipe Ends."]
["\n\n302 Series\nBronze ","\nClick picture for detailed info","1/2\"","Silver Braze","147 mm","-196°C \n\nto \n\n+65°C","28 Barg\n\n400PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Micro Bulk\n\nBulk Tanks\n\nTrailers\n\nPipelines","   \n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n   Split wedge Bronze\n   Replaceable\n\n   Metal Seat\n"]
[null,null,"3/4\"",null,"176 mm"]
[null,null,"1\"",null,"214 mm"]
[null,null,"\n1 1/2\"\n",null,"284 mm"]
[null,null,"\n2\"\n",null,"335 mm"]
[null,null,"2 1/2\"",null,"401 mm"]
[null,null,"3\"",null,"463 mm"]
[null,"\nClick picture for detailed info","1/2\"","Threaded","147 mm"]
[null,null,"2 1/2\"",null,"401 mm"]
[null,null,"3\"",null,"463 mm"]
["    306 Series Bronze Gate Valve - Non Extended Stem, Metal Seated, with End Connections:  Threaded Ends."]
[null,"\nClick picture for detailed info","3/4\"","Threaded","176 mm","-196°C \n\nto \n\n+65°C","42 Barg\n\n600PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Micro Bulk\n\nBulk Tanks\n\nTrailers\n\nPipelines","   \n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n   Split wedge Bronze\n   Replaceable\n\n   Metal Seat\n"]
[null,null,"1\"",null,"214 mm"]
[null,null,"\n1 1/2\"\n",null,"284 mm"]
[null,null,"\n2\"\n",null,"335 mm"]
["    310 Series Bronze Gate Valve - Extended Stem, Soft Seated, with End Connections:  Threaded Ends  -  Silver Braze Ends."]
[null,"\nClick picture for detailed info","\n 3\"","Silver Braze","\n 645 mm","-198°C to + 65°C","20 Barg\n\n300PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Bulk Tank\n\nTrailers\n\nPipelines","   Solid wedge with \n   PCTFE (Neoflon ) \n   provides a bubble tight \n   seal and is replaceable.\n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested"]
[null,"\nClick picture for detailed info"," 2 1/2\"","Threaded","645 mm\n"]
[null,null,"\n3\"",null,"645 mm"]
["    310X Series Bronze Gate Valve - Extended Stem, Soft Seated, with End Connections: Pipe ends SCH10 - Pipe ends SCH40"]
[null,"\nClick picture for detailed info"," 2 1/2\"","Pipe Ends SCH10","\n 518 mm","-198°C to + 65°C","20 Barg\n\n300PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Bulk Tank\n\nTrailers\n\nPipelines","   Solid wedge with \n   PCTFE (Neoflon ) \n   provides a bubble tight \n   seal and is replaceable.\n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested"]
[null,null,"\n3\"",null,"645 mm\n"]
[null,null,"\n3\"","Pipe Ends SCH40","645 mm\n"]
["    310X Series Bronze Gate Valve - Short Topwork - Trailer Service, Soft Seated, with End Connections:  Threaded Ends  -  Silver Braze Ends."]
[null,"\nClick picture for detailed info","\n 3\"","Silver Braze","518 mm","-198°C to + 65°C","20 Barg\n\n300PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Trailers","   Solid wedge with \n   PCTFE (Neoflon ) \n   provides a bubble tight \n   seal and is replaceable.\n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested"]
[null,null," 2 1/2\"","Threaded","518 mm"]
[null,null,"3\"","Threaded","518 mm"]
["SB-00310X-24SW\n\nStainless Steel Body\n+\nBronze Topwork","\nClick picture for detailed info","\n 3\"","Socket weld","518 mm"]
["    322 - 326 Series Bronze Gate Valve, with End Connections:  Threaded Ends  -  Silver Braze Ends  -  Stainless Steel Pipestubs."]
["\n322 Series","\nClick picture for detailed info","1/2\"","Silver Braze","238 mm","-196°C \n\nto \n\n+65°C","28 Barg\n\n400PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Micro Bulk\n\nBulk Tanks\n\nTrailers\n\nPipelines","   \n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\n  Metal Seat\n"]
[null,null,"3/4\"",null,"268 mm"]
[null,null,"1\"",null,"314 mm"]
[null,null,"\n1 1/2\"\n",null,"432 mm"]
[null,null,"\n2\"\n",null,"498 mm"]
[null,null,"2 1/2\"",null,"571 mm"]
[null,null,"3\"",null,"632 mm"]
[null,"\nClick picture for detailed info","2 1/2\"","Threaded ","571 mm"]
[null,null,"3\"",null,"632 mm"]
["\n326 Series","\nClick picture for detailed info","1/2\"","Threaded ","238 mm","-196°C \n\nto \n\n+65°C","42 Barg\n\n600PSIG","Oxygen\n\nNitrogen\n\nArgon\n\nCO2\n\nNatural Gas","LOX\n\nLIN\n\nLAR\n\nLCO2\n\nLNG","PED\n\nCRN Registration","Micro Bulk\n\nBulk Tanks\n\nTrailers\n\nPipelines","   \n\n   Cleaned for use in \n   Oxygen per CGA G-4.1\n\n   100% Factory Tested\n\nMetal Seat\n"]
[null,null,"3/4\"",null,"268 mm"]
[null,null,"1\"",null,"314 mm"]
[null,null,"\n1 1/2\"\n",null,"432 mm"]
[null,null,"\n2\"\n",null,"498 mm"]

{"sheet":"110 Series","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"110WHZ Series","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"110 LOX Series","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"302-306 Series","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"310-310X Series","index":5,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":false,"merged":[[0,8,5,9],[2,1,3,6]]}
[]
[]
[null,"Note: SB-320X-24SW  =  Stainless Steel Body & Bronze Topwork"]

{"sheet":"322 & 326 Series","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}